Attunity® Integration Suite

Installation Guide for Mainframe Systems

Version 5.3.4

January 2016

Attunity Integration Suite Installation Guide for Mainframe Systems, Version 5.3.4

Copyright © Januaryy 2016 Attunity Ltd. All rights reserved.

Primary Authors: Andre Liss, Amitai Sela, David Goldman

Contributors: Meera Srinivasan, Deanna Bradshaw, Yishai Hadas, Dror Harari, Arvind Jain, Pratibha

Singhal, Mark Kennedy, Adeeb Massad, Bo Stern, Costi Zaboura

The Programs (which include both the software and documentation) contain proprietary information; they

are provided under a license agreement containing restrictions on use and disclosure and are also protected

by copyright, patent, and other intellectual and industrial property laws. Reverse engineering, disassembly,

or decompilation of the Programs, except to the extent required to obtain interoperability with other

independently created software or as specified by law, is prohibited.

The information contained in this document is subject to change without notice. If you find any problems in

the documentation, please report them to us in writing. This document is not warranted to be error-free.

Except as may be expressly permitted in your license agreement for these Programs, no part of these

Programs may be reproduced or transmitted in any form or by any means, electronic or mechanical, for any

purpose.

If the Programs are delivered to the United States Government or anyone licensing or using the Programs on

behalf of the United States Government, the following notice is applicable:

U.S. GOVERNMENT RIGHTS Programs, software, databases, and related documentation and technical data

delivered to U.S. Government customers are "commercial computer software" or "commercial technical data"

pursuant to the applicable Federal Acquisition Regulation and agency-specific supplemental regulations. As

such, use, duplication, disclosure, modification, and adaptation of the Programs, including documentation

and technical data, shall be subject to the licensing restrictions set forth in the applicable Attunity license

agreement, and, to the extent applicable, the additional rights set forth in FAR 52.227-19, Commercial

Computer Software--Restricted Rights (June 1987).

The Programs are not intended for use in any nuclear, aviation, mass transit, medical, or other inherently

dangerous applications. It shall be the licensee's responsibility to take all appropriate fail-safe, backup,

redundancy and other measures to ensure the safe use of such applications if the Programs are used for such

purposes, and we disclaim liability for any damages caused by such use of the Programs.

The Programs may provide links to Web sites and access to content, products, and services from third

parties. Attunity is not responsible for the availability of, or any content provided on, third-party Web sites.

You bear all risks associated with the use of such content. If you choose to purchase any products or services

from a third party, the relationship is directly between you and the third party. Attunity is not responsible

for: (a) the quality of third-party products or services; or (b) fulfilling any of the terms of the agreement with

the third party, including delivery of products or services and warranty obligations related to purchased

products or services. Attunity is not responsible for any loss or damage of any sort that you may incur from

dealing with any third party.

iii

Contents

1 Pre-installation and Upgrade Notes

What Steps are Performed for an Installation or an Upgrade ......................................................... 1-1

2 Installation and Configuration

IBM z/OS Hardware and Software Requirements ............................................................................ 2-1

Hardware Requirements................................................................................................................... 2-1

Software Requirements ..................................................................................................................... 2-1

Installing Attunity Server on an IBM z/OS Series Platform ........................................................... 2-2

Installation Worksheet....................................................................................................................... 2-2

Preinstallation Instructions............................................................................................................... 2-3

Kit Installation Instructions .............................................................................................................. 2-3

Transferring the Kit to the Dataset ........................................................................................... 2-4

Installation Instructions..................................................................................................................... 2-4

Data Source Configuration Instructions ......................................................................................... 2-7

Postinstallation Instructions ............................................................................................................. 2-9

Copy and Install Programs into CICS...................................................................................... 2-9

Postinstallation Procedures .................................................................................................... 2-11

Starting the Daemon................................................................................................................ 2-12

Setting Up Attunity Server for Reentrancy .......................................................................... 2-12

Updating an Existing Attunity Server Installation with CICS..................................................... 2-13

3 Post-Installation Instructions

Overview.................................................................................................................................................... 3-1

General Post Installation Procedures ................................................................................................... 3-2

Registering Attunity Server .............................................................................................................. 3-2

Setting APF-Authorization and Started Tasks............................................................................... 3-2

Setting 2-Phase Commit.................................................................................................................... 3-4

TCP/IP................................................................................................................................................. 3-4

Workspace for z/OS Server Environment File.............................................................................. 3-4

Setting Up Security .................................................................................................................................. 3-5

Attunity Server Stream and DB2 Security...................................................................................... 3-6

Setting Up Attunity Server to Work with CICS ................................................................................. 3-6

Setting Up Attunity Server to Work with IMS/TM........................................................................... 3-7

Setting up Attunity Server to work with IMS/DB CDC.............................................................. 3-8

Setting Up Attunity Server for Reentrancy......................................................................................... 3-8

iv

Setting Up Attunity Server to Access DB2 CLI .................................................................................. 3-8

Setting Up Attunity Server to Update VSAM Data........................................................................... 3-9

Setting Up Attunity Server to Access IMS/DB................................................................................... 3-9

Setting Up IMS/DB Under IMS/TM ........................................................................................... 3-10

Installing Attunity Server Natural/CICS Agent.............................................................................. 3-10

Configuring the Agent ................................................................................................................... 3-11

Installing the CICS Resource Definitions .................................................................................... 3-11

Loading and Cataloging the Natural Programs ......................................................................... 3-12

Making the Agent Load Modules Available to the CICS Region ............................................ 3-12

Verifying the Agent Installation is Successful ............................................................................ 3-13

Verifying the Installation is Successful from a Client................................................................ 3-14

Setting the Language ............................................................................................................................ 3-15

Index

Pre-installation and Upgrade Notes 1-1

1

Pre-installation and Upgrade Notes

This section includes Attunity Server pre-installation requirements for z/OS and

upgrade notes.

What Steps are Performed for an Installation or an Upgrade

Before starting the installation, make sure that you have the following information

available, which is prompted for during the installation:

n The output class for the installation output if you don’t want to use the default.

n To enable access to DB2:

n The DB2 database high-level qualifier.

n The name of the DB2 subsystem identifier name.

n To enable access to Adabas:

n The Adabas SVC number (the default is 249).

n The Adabas database number.

n The Adabas load library location (the default is ADA622.LOAD)

1-2 Attunity Integration Suite Installation Guide for Mainframe Systems

Installation and Configuration 2-1

2

Installation and Configuration

This section describes how to install to configure Attunity Server using Attunity

Studio.

This section includes the following topics:

n IBM z/OS Hardware and Software Requirements

n Installing Attunity Server on an IBM z/OS Series Platform

n Updating an Existing Attunity Server Installation with CICS

IBM z/OS Hardware and Software Requirements

This section describes the following requirements for installing Attunity Server on an

IBM z/OS platform:

n Hardware Requirements

n Software Requirements

Hardware Requirements

The following table summarizes the hardware requirements for Attunity Server:

Software Requirements

The following table summarizes the software requirements for Attunity Server:

Hardware Component Requirements

Processor An IBM zSeries computer

Disk Space (3390 disk) 150 cylinders

Software Component Requirements

Operating System See the customer support section at www.attunity.com

for the currently supported operating systems and

versions.

TCP/IP TCP/IP needs to be active on the system.

C Runtime Library The C runtime library has all the standard C runtime programs.

2-2 Attunity Integration Suite Installation Guide for Mainframe Systems

Installing Attunity Server on an IBM z/OS Series Platform

This section explains how to install Attunity Server. This section includes the

following:

n Installation Worksheet

n Preinstallation Instructions

n Kit Installation Instructions

n Installation Instructions

n Data Source Configuration Instructions

n Postinstallation Instructions

Installation Worksheet

Verify that you have all the information detailed in the following installation

worksheets, so you can refer to it during the configuration process.

Note: If you have an AIS back-end adapter already installed on

the IBM z/OS platform, then follow the instructions described in

Updating an Existing Attunity Server Installation with CICS on

page 2-13.

Table 2–1 Preinstallation Information

Topic Required Information Default Comment

General Operating system - See the customer support section at

www.attunity.com for the currently

supported operating systems and

versions.

- Disk space - 150 cylinders

- Installation high-level

qualifier

- -

- Volume - -

- Unit 3390 SMS only: unit where SMS resides.

- Output class A -

- JCL job card - An optional card (up to 6 lines) to replace

the prefix job (entered as it will appear in

the job)

- ISPF load library name ISP.SISPLOAD -

CICS CICS EXCI load library name CICS.CICS.SDFHEXCI -

Table 2–2 Required Permissions

Permission

Permission to define an APF-authorized library

Permission to write to an active proclib, such as user.proclib

Installation and Configuration 2-3

Preinstallation Instructions

Before starting the installation, ensure that the following information is available:

n The output class for the installation output if you do not want to use the default

value, which is A.

Before starting the installation, ensure that you have the following permissions:

n Permission to define an APF-authorized library.

n Permission to write to an active proclib, such as user.proclib.

n Permission to read the CICS EXCI library.

n Permission to update the security manager, such as RACF

Attunity Server for the IBM z/OS platform is contained in the following datasets:

n <HLQ>.TRANSMIT.KIT

n <HLQ>.TRANSMIT.LOAD

Kit Installation Instructions

Perform the following on the mainframe:

1. Run the following command:

Permission to read the CICS EXCI library

Permission to update the security manager, such as RACF

Optionally, permission to specify an output class for Attunity Server output

Table 2–3 Installation Checklist

Step Comment/Outputs

tso profile noprefix Ensures that the user name is not used as part of

the dataset name allocated in the next steps

Allocate dataset: {HLQ}.TRANSMIT.KIT 130 tracks (3390), format=FB, record length=80,

block size=3120

Allocate dataset: {HLQ}.TRANSMIT.LOAD 600 tracks (3390), format=FB, record length=80,

block size=3120

FTP files to z/OS FTP using binary mode

RECEIVE INDSNAME('{HLQ}.TRANSMIT.KIT') -

da('{HLQ}.TRANSMIT.LIB') UNIT(unit) VOLUME(volume) -

EX {HLQ}.TRANSMIT.LIB(PREPARE) Successful MAXCC is 0, 4 or 8

BUILDKIT.SRC, BUILDKIT.LOAD, and

BUILDKIT.GENDEMO created

EX {HLQ}.BUILDKIT.SRC(NAVINST) Successful MAXCC is 0 or 4

Note: It is recommended to specify an output class with HOLD

status to prevent the loss of Attunity Server log information.

Table 2–2 (Cont.) Required Permissions

Permission

2-4 Attunity Integration Suite Installation Guide for Mainframe Systems

tso profile noprefix

The user name will not be used as part of the dataset name. On some systems this

is the default.

2. If HLQ does not exist, you might want to define an alias for it now.

3. Allocate datasets with the following space for each of these files:

n [HLQ].TRANSMIT.KIT = 130 tracks (3390 disk)

n [HLQ].TRANSMIT.LOAD = 600 tracks (3390 disk)

For each dataset: RECFM=FB, LRECL=80 and DSORG=PS. The block size is 3120.

Transferring the Kit to the Dataset

You need to copy the contents of the kit to the z/OS datasets just allocated.

Perform the following steps to copy the AIS installation kit contents to the mainframe:

1. Extract the compressed file to a folder on your computer.

2. Perform the transfer using one of the following methods:

Method 1:

If you have a standard procedure for file transfer, use it to perform a binary

transfer of the following files:

n ac5340.transmit.kit to '[HLQ].transmit.kit'

n ac5340.transmit.load to '[HLQ].transmit.load'

Method 2:

a. Open a Windows command prompt.

b. Type FTP followed by a space and the name of the z/OS to which you wish to

connect. This creates an FTP connection to the mainframe machine. Enter your

z/OS userid and password when prompted for them.

c. Type bin to indicate a binary transfer.

d. Enter the following command to transfer the data from the .KIT file to z/OS:

put ac5340.transmit.kit '[HLQ].transmit.kit' [replace]

Where:

– ac5340.transmit.kit is the name of your installation file on Windows

– [replace] overwrites the old installation dataset on z/OS (should one

exist)

e. Enter the following command to transfer the data from the .LOAD file o z/OS:

put ac5340.transmit.load '[HLQ].transmit.load' [replace]

f. Exit FTP by typing quit.

Installation Instructions

Perform the following steps to install Attunity Server:

1. Run the following command in the Data Set List screen.

TSO RECEIVE INDSNAME('<HLQ>.TRANSMIT.KIT')

Installation and Configuration 2-5

Where <HLQ> represents the high-level qualifier that you assign for the Attunity

Server installation. Assign the high-level qualifier you used in the preinstallation

procedure.

2. Enter the following when prompted for the restore parameters:

da('<HLQ>.TRANSMIT.LIB') [UNIT(unit) VOLUME(volume)]

This extracts the <HLQ>.TRANSMIT.LIB library from the <HLQ>.TRANSMIT.KIT

kit to the specified unit and volume. If a unit and volume are not specified then

the library is extracted to the default unit and volume.

3. Enter the following TSO command:

TSO EX '<HLQ>.TRANSMIT.LIB(PREPARE)'

Follow the instructions in the Response column in Table 2–4 for each entry in the

Screen column.

Note: You can use more than one high-level qualifier, such as

ACME.DEV.<HLQ>, with the following conditions:

n The total length must be less than or equal to twenty characters.

n The words transmit and buildkit cannot be used as high-level

qualifiers.

Table 2–4 Installation Prepare Job Prompts and Responses

Screen Response

DO YOU WANT TO USE SMS MANAGED

STORAGE FOR THIS INSTALLATION Y/N [N] :

If you want to manage the storage using SMS, then answer

Y, otherwise answer N.

ENTER THE STORCLASS FOR INSTALLATION

TEMP DATASETS [ ] :

This prompt is displayed only if SMS is used to manage the

installation (you answered Y to the first prompt).

Enter the storage class

ENTER THE UNIT NAME FOR INSTALLATION

TEMP DATASETS [3390] :

If a storage class is not specified, then enter the unit name

for temporary datasets used during the installation

procedure

ENTER THE VOLUME NAME FOR

INSTALLATION TEMP DATASETS :

This prompt is displayed only if SMS is not used to manage

the installation (you answered N to the first prompt).

The volume name for temporary datasets used during the

installation procedure

ENTER THE OUTPUT CLASS FOR

INSTALLATION OUTPUT [A] :

Enter the output class only if you do not want the default

class used (the default is A)

2-6 Attunity Integration Suite Installation Guide for Mainframe Systems

4. Verify that all steps on the INSTJO job ended with return code 0.

5. Enter the following TSO command:

TSO EX '<HLQ>.BUILDKIT.SRC(NAVINST)'

Follow the instructions in the Response column in Table 2–5 for each entry in the

Screen column.

DO YOU WANT TO USE THE DEFAULT JOB

CARD Y/N [Y]

A job card is displayed. If you want to use a replacement

card, then it must be entered as it will appear in the job. You

can enter up to six lines. Enter a blank card to end input.

If you do not enter a card, then the Attunity Server default

card is used.

DO YOU WANT TO PERFORM A MANUAL

(M) OR AUTOMATIC (A) INSTALLATION [A] :

If you want to review the JCL used to install Attunity

Server, before it is submitted, then respond M for a manual

installation.

PLEASE REVIEW AND SUBMIT FOR

EXECUTION THE

HLQ.TRANSMIT.LIB(INSTJO)

This prompt is displayed only if a manual installation is

requested (you answered M to the previous prompt).

Table 2–5 Installation Prompts and Responses

Screen Response

DO YOU WANT TO USE SMS MANAGED

STORAGE FOR THIS INSTALLATION Y/N [N]:

If you want to manage the storage using SMS, then answer

Y, otherwise answer N.

THE SOFTWARE WILL BE INSTALLED UNDER

THE HIGH LEVEL QUALIFIER THAT YOU

WILL CHOOSE.

ENTER THE HIGH LEVEL QUALIFIER

["QUALIFIER"]:

The high-level qualifier for the installation (referred to as

INSTROOT throughout this guide)

You can use more than one high-level qualifier (such as

ACME.DEV.VA10). The total length must be less than or

equal to twenty characters. The qualifiers can be the same

as the ones used for the installation (step 1).

The words transmit and buildkit cannot be used as

high-level qualifiers.

ENTER THE STORCLASS FOR TEMP DATASETS

['STORCLASS']:

This prompt is displayed only if SMS is used to manage the

installation (you answered Y to the first prompt).

Enter the storage class

ENTER THE UNIT NAME FOR INSTALLATION

TEMP DATASETS [3390] :

The unit name for temporary datasets used during the

installation procedure.

ENTER THE VOLUME NAME FOR

INSTALLATION TEMP DATASETS:

This prompt is displayed only if SMS is not used to manage

the installation (you answered N to the first prompt).

The volume name for temporary datasets used during the

installation procedure

PLEASE CONFIRM (YES/NO/QUIT) [YES]: Confirm the entered details

ENTER THE OUTPUT CLASS FOR

INSTALLATION OUTPUT [A]:

Enter the output class for Attunity Server output. Assigning

a device which is set on HOLD prevents the loss of log

information when the Attunity Server started tasks finish

(the default is A).

Table 2–4 (Cont.) Installation Prepare Job Prompts and Responses

Screen Response

Installation and Configuration 2-7

The installation is completed. All JCL jobs and REXX procedures are written to the

INSTROOT.USERLIB library. INSTROOT is the high-level qualifier for the installation.

Data Source Configuration Instructions

Enter the following TSO command:

TSO EX '<HLQ>.BUILDKIT.SRC(CUST)'

Follow the instructions in the Response column in Table 2–6 for each entry in the

Screen column.

ADDING AND UPDATING ATTUNITY

CONNECT FOR CICS CONFIGURATION ON

THIS MACHINE, FROM A REMOTE ATTUNITY

ADMINISTRATION CONSOLE, CAN ONLY BE

DONE BY SOMEONE DEFINED AS AN

ADMINISTRATOR FOR ATTUNITY CONNECT

ON THIS MACHINE.

ENTER A VALID USER NAME FOR AN

ATTUNITY CONNECT ADMINISTRATOR

[ALL]:

In order to manage Attunity Server on this computer from

Attunity Studio, you need to enter a user account of a user

who will have administrative authorization, or press Enter

to enable any user to administer Attunity Server on this

computer. The administrative rights can be changed from

within Attunity Studio after the installation.

DO YOU WANT TO USE THE DEFAULT JOB

CARD Y/N [Y]

A job card is displayed. If you want to use a replacement

card, then it must be entered as it will appear in the job. You

can enter up to six lines. Enter a blank card to end input.

If you do not enter a card, then the Attunity Server default

card is used.

DO YOU WANT TO PERFORM A MANUAL (M)

OR AUTOMATIC (A) INSTALLATION [A] :

If you want to review the JCL used to install Attunity

Server, before it is submitted, then respond M for a manual

installation.

PLEASE REVIEW AND SUBMIT FOR

EXECUTION THE DSN1 (INSTJBOR)

This prompt is displayed only if a manual installation is

requested (you answered M to the previous prompt).

DSN1 is the dataset name where INSTJBOR is located.

Table 2–6 Installation Prompts and Responses

Screen Response

DO YOU WANT ATTUNITY SERVER TO WORK

WITH DB2

If you want to use DB2, then answer Y, otherwise answer N

ENTER THE DB2 HLQ This is displayed only if you answered Y to using DB2. Enter

the HLQ where DB2 is installed.

ENTER THE DB2 SUBSYSTEM NAME Enter the DB2 subsystem.

THE DATABASE DB2 RESIDES ON THIS

MACHINE

THE DB2 SUBSYSTEM NAME IS :

PLEASE CONFIRM (YES/NO/QUIT) :YES: :

This is a summary of the DB2 questions. Check the

summary to be sure all is correct. You can select:

n Yes, to use the DB2 database as configured

n No, to not use the DB2 database

n Quit, to leave the CUST process

DO YOU WANT ATTUNITY SERVER TO WORK

WITH ADABAS

If you want to use Adabas, then answer Y, otherwise answer

N.

ENTER THE ADABAS SVC NUMBER This is displayed only if you answered Y to using Adabas.

Enter the Adabas SVC number for Adabas on your system.

Table 2–5 (Cont.) Installation Prompts and Responses

Screen Response

2-8 Attunity Integration Suite Installation Guide for Mainframe Systems

ENTER THE ADABAS LOAD LIBRARY NAME Enter the Adabas Load Library name for Adabas on your

system.

YOUR ADABAS SVC IS:

THE ADABAS LOAD LIBRARY NAME IS:

PLEASE CONFIRM (YES/NO/QUIT)

This is a summary of the Adabas questions. Check the

summary to be sure all is correct. You can select:

n Yes, to use the Adabas database as configured

n No, to not use the Adabas database

n Quit, to leave the CUST process

DO YOU WANT ATTUNITY SERVER TO WORK

WITH IMS

If you want the server to work with IMS, then answer Y,

otherwise answer N.

ENTER IMS ID [IMS1]: Enter the IMS subsystem ID

ENTER DBD LIBRARY NAME Enter the IMS DBD Library name for IMS on your system

ENTER PSB LIBRARY NAME Enter the IMS PSB Library name for IMS on your system

ENTER RES LIBRARY NAME Enter the IMS RES Library name for IMS on your system

ENTER PROC LIBRARY NAME Enter the IMS PROC Library name for IMS on your system

ENTER PGM LIBRARY NAME Enter the IMS PGM Library name for IMS on your system.

ENTER YOUR PSB NAME Enter the name of the PSB file with the name of your IMS

database.

YOUR DBDLIB IS:

YOUR PSBLIB IS:

YOUR RESLIB IS:

YOUR PROCLIB IS:

YOUR PGMLIB IS:

YOUR PSBNAME IS:

PLEASE CONFIRM (YES/NO/QUIT) :YES: :

This is a summary of the IMS questions. Check the summary

to be sure all is correct. You can select:

n Yes, to use the IMS database as configured

n No, to not use the IMS database

n Quit, to leave the CUST process

DO YOU WANT ATTUNITY SERVER TO WORK

WITH IMS/DB UNDER CICS

f you want the server to work with IMS/DB under CICS,

then answer Y, otherwise answer N.

ENTER THE CICS EXCI LOAD LIBRARY NAME

[CICSTS13.CICS.SDFHEXCI]:

Enter the CICS EXCI load library name only if you do not

want the default

PLEASE CONFIRM (YES/NO/QUIT) [YES]: Confirm the entered details

DO YOU WANT ATTUNITY SERVER TO WORK

WITH CICS APP ADAPTER

f you want the server to work with the CICS APP

ADAPTER, then answer Y, otherwise answer N.

ENTER THE ISPF LOAD LIBRARY NAME

[ISP.SISPLOAD] :

Enter the ISPF load library name only if you do not want the

default

PLEASE CONFIRM (YES/NO/QUIT) [YES]: Confirm the entered details

Table 2–6 (Cont.) Installation Prompts and Responses

Screen Response

Installation and Configuration 2-9

Postinstallation Instructions

The following postinstallation tasks must be done to work with Attunity Server:

n Copy and Install Programs into CICS

n Postinstallation Procedures

n Starting the Daemon

n Setting Up Attunity Server for Reentrancy

Copy and Install Programs into CICS

You must copy and install the some supporting programs if you are using a CICS

session. The following table describes the programs and when you must use them.

The following describes the steps necessary to copy and install these programs under

CICS.

1. In the Data Set List Utility screen, type the name of the <HLQ> on the Dsname

Level line. This will return a list of the files.

2. In the Command column next to the <HLQ>.LOAD, type M.

ENTER THE OUTPUT CLASS FOR

INSTALLATION OUTPUT [A]:

Enter the output class for Attunity Server output. Assigning

a device which is set on HOLD prevents the loss of log

information when the Attunity Server started tasks finish

(the default is A).

DO YOU WANT TO USE THE DEFAULT JOB

CARD Y/N [Y]

A job card is displayed. If you want to use a replacement

card, then it must be entered as it will appear in the job. You

can enter up to six lines. Enter a blank card to end input.

If you do not enter a card, then the Attunity Server default

card is used.

DO YOU WANT TO PERFORM A MANUAL

(M) OR AUTOMATIC (A) CUSTOMIZATION :A:

It is recommended that you choose automatic, which is the

default.

Table 2–7 CICS Programs

Program When to use it

ATYGTEVT Use this program when working with CICS. This is the CICS

queue.

ATTCICSD Use this program when working with CICS.

ATTHRDPL Use this program when working with CICS, if you are using

connection pooling.

ATTCALL Use this program when working with CICS, if you are using

connection pooling.

ATTCNTRL Use this program when working with CICS, if you are using

connection pooling.

ATYDBCTL Use this program if you are using the IMS CDC agent.

TRANS3GL Use this program if you are using the 3GL interface. This is an

sample program.

UPDTRNS Use this program if you are using the VSAM CDC agent.

Table 2–6 (Cont.) Installation Prompts and Responses

Screen Response

2-10 Attunity Integration Suite Installation Guide for Mainframe Systems

3. Type C next to the programs that you wish to use. The list of available programs is

in the CICS Programs table.

4. Hit the <enter> key and specify the name of the target CICS load library (One

concatenated to the DFHRPL DD statement).

5. Log on to CICS.

6. Enter the following transaction:

CEDA INS PROG(<PROG NAME>) G(ATY)

The <PROG NAME> is on one of the programs from the CICS Programs table. Run this

for each of the programs you are using.

Installation and Configuration 2-11

Postinstallation Procedures

After installation, the following steps are required:

n Copy ATTDAEMN from <HLQ>.USERLIB to a system procedure library (such as

SYS1.PROCLIB) and edit the following line as required:

// PARM='-B -L <ip\_address>:<port> START IRPCDINI'

Where ip\_address is ip address of the computer, 2551 is the default port for

starting the daemon and IRPCDINI is the default daemon configuration.

n Copy <HLQ>.USERLIB (ATTSRVR) to a system procedure library (such as

SYS1.PROCLIB). If you are using IMS, copy NVIMSSRV and NVBMPSRV as well.

If you decide to change the name of the ATTSRVR member when you move it to a

general high-level qualifier, then change the name specified in the

StartupScript parameter in the daemon configuration to the new name:

n Run <HLQ>.USERLIB(NAVCMD) and enter EDIT DAEMON IRPCDINI at the

prompt.

n Change the startupScript parameter from ATTSRVR to the new name for the

server:

<Workspace name="Navigator"

startupScript="NEW\_NAME"

serverMode="reusable"

... />

n Exit and save the changes.

n Define the LOADAUT library as an APF-authorized library.

If RRS is going to be used, define LOAD library as APF-authorized.

Ask your z/OS system programmer to add <HLQ>.LOADAUT as an

APF-authorized library.

n Using your security manager (such as RACF), assign a user to the following

started tasks: ATTDAEMN, ATTSRVR and NVIMSSRV (if you are using IMS/DLI).

The user should have the following authority:

n Permission to issue master console commands.

n Permission to start ATTSRVR.

n Access to an OMVS segment.

n ALTER authority on datasets under INSTROOT to access to read, write,

allocate, and delete datasets under INSTROOT.

n The input during the installation procedure is written to

nnn.BUILDKIT.SRC(PARS). You can use this file to provide the same inputs if

you rerun the installation, where nnn is the high-level qualifier you assign for the

installation.

n For information about specifying Attunity Server as the service using port 2551 in

the TCP/IP configuration parameters, refer to z/OS Communications Server IP

Configuration Reference.

2-12 Attunity Integration Suite Installation Guide for Mainframe Systems

Starting the Daemon

Start the daemon by issuing the following z/OS command:

S ATTDAEMN

If you have changed the name of the started task, use the new name instead of

ATTDAEM.

To submit the daemon as a job, uncomment the first two lines of the ATTDAEMN JCL,

change the PARM line as described earlier, and run the job using the subcommand.

The ATTDAEMN JCL is similar to the following:

//\*ATTDAEMN JOB 'RR','TTT',MSGLEVEL=(1,1),CLASS=A,

//\* MSGCLASS=A,NOTIFY=&SYSUID,REGION=8M

//STEP1 EXEC PGM=IRPCD,

// PARM='-B START IRPCDINI'

//\* PARM='-B -L :8883 START'

//STEPLIB DD DSN=INSTROOT.LOADAUT,DISP=SHR

//SYSPRINT DD SYSOUT=A

//GBLPARMS DD DSN=INSTROOT.DEF.GBLPARMS,DISP=SHR

// EXEC PGM=IRPCD,COND=((1,EQ,STEP1),(2,EQ,STEP1)),

// PARM='-KATTDAEMN START ''INSTROOT.DEF.IRPCDINI'''

//STEPLIB DD DSN=INSTROOT.LOADAUT,DISP=SHR

//SYSPRINT DD SYSOUT=A

//GBLPARMS DD DSN=INSTROOT.DEF.GBLPARMS,DISP=SHR

//SYSDUMP DD DUMMY

Setting Up Attunity Server for Reentrancy

All Attunity Server load modules are reentrant and therefore eligible for LPA. Placing

these modules in the LPA improves response time and saves virtual memory. It is

recommended to place INSTROOT.LOA in the LPA concatenation. Ask your z/OS

programmer to do this.

Note: When the language is set to JPN, KOR, SPA, or SCHI, the

daemon may stop responding. To be sure that the daemon responds

add HLQ.LOAD to the STEPLIB. To do this, add:

DD DSN=HLQ.LOAD

to the end of the following line:

//STEPLIB DD DSN=INSTROOT.LOADAUT,DISP=SHR

Note: If you intend using impersonation, so that you can run in a

security context that is different than the context of the process that

owns the server, then do the following:

n Place the INSTROOT.LOAD(ATYSVCW) member in an

APF-authorized library outside the LPA.

n Change the ATTSRVR member (located in the active proclib), by

adding the following to the STEPLIB list:

// DD DSN=apf\_library,DISP=SHR

Where apf\_library is the APF-authorized library outside the

LPA where the ATYSCVW member was moved.

Installation and Configuration 2-13

Updating an Existing Attunity Server Installation with CICS

Verify that you have all the information detailed in the following installation

worksheets, so you can refer to it during the configuration process.

In the nnn.BUILDKIT.SRC library, run the CUST member, as shown:

ex CUST

Follow the instructions in the Response column in Table 2–10 for each entry in the

Screen column.

Table 2–8 Preinstallation Information

Topic Required Information Default Comment

CICS CICS EXCI load library name CICS.CICS.SDFHEXCL -

Table 2–9 Required Permissions

Permission

Permission to read the CICS EXCI library

Table 2–10 CICS Adapter Installation Prompts and Responses

Screen Response

DO YOU WANT ATTUNITY CONNECT FOR

LEGACY ADAPTER TO WORK WITH IMS/DB

(YES/NO) [YES] :

Answer YES to this prompt if you have AIS for IMS/DB

already installed.

ENTER DBD LIBRARY NAME [IMS.DBDLIB] : If you responded YES to working with IMS/DB, then enter

the library where database definition (DBD) files are located.

ENTER PSB LIBRARY NAME [IMS.PSBLIB] : If you responded YES to working with IMS/DB, then enter

the library where Program Specification Blocks (PSBs) are

located.

ENTER YOUR PSB NAME [HOSPPSB] : If you responded YES to working with IMS/DB, then enter

the name of the PSB file to use.

PLEASE CONFIRM (YES/NO/QUIT) [YES] : If you responded YES to working with IMS/DB, then

confirm the entered details.

DO YOU WANT ATTUNITY CONNECT FOR

LEGACY ADAPTER TO WORK WITH IMS/DB

UNDER CICS (YES/NO) [NO] :

If you want to access IMS/DB data under CICS, using AIS

adapter for IMS/DB, then respond YES.

ENTER THE CICS EXCI LOAD LIBRARY NAME

[CICSTS13.CICS.SDFHEXCI] :

If you responded YES to working with IMS/DB under CICS,

then enter the CICS EXCI load library name only if you do

not want the default.

PLEASE CONFIRM (YES/NO/QUIT) [YES] : If you responded YES to working with IMS/DB under CICS,

then confirm the entered details.

DO YOU WANT ATTUNITY CONNECT FOR

LEGACY ADAPTER TO WORK WITH CICS

APP ADAPTER (YES/NO) [YES] :

Answer YES to this prompt

ENTER THE CICS EXCI LOAD LIBRARY NAME

[CICSTS13.CICS.SDFHEXCI] :

Enter the CICS EXCI load library name only if you do not

want the default.

PLEASE CONFIRM (YES/NO/QUIT) [YES] : Confirm the entered details

2-14 Attunity Integration Suite Installation Guide for Mainframe Systems

The installation is completed. All JCL jobs and REXX procedures are written to the

INSTROOT.USERLIB library. INSTROOT is the high-level qualifier for the installation.

After completing the installation, perform postinstallation tasks, as described in

"Post-Installation Instructions", as required.

THE VSAM DRIVER IS INSTALLED

AUTOMATICALLY. DO YOU ALSO WANT

ATTUNITY CONNECT FOR LEGACY

ADAPTER TO WORK WITH VSAM UNDER

CICS (YES/NO) [NO] :

Answer YES to this prompt if you have AIS for VSAM

already installed and you want to access VSAM data under

CICS.

ENTER THE CICS EXCI LOAD LIBRARY NAME

[CICSTS13.CICS.SDFHEXCI] :

If you responded YES to working with VSAM under CICS,

then enter the CICS EXCI load library name only if you do

not want the default.

PLEASE CONFIRM (YES/NO/QUIT) [YES] : If you responded YES to working with VSAM under CICS,

then confirm the entered details.

ENTER THE ISPF LOAD LIBRARY NAME

[ISP.SISPLOAD] :

Enter the ISPF load library name only if you do not want the

default.

PLEASE CONFIRM (YES/NO/QUIT) [YES] : Confirm the entered details

ENTER THE OUTPUT CLASS FOR

INSTALLATION OUTPUT [A] :

Enter the output class for the Attunity Server output.

Assigning a device which is set on HOLD prevents the loss of

log information when the Attunity Server started tasks

finish (the default is A).

DO YOU WANT TO USE THE DEFAULT JOB

CARD Y/N [Y]

A job card is displayed. If you want to use a replacement

card, then it must be entered as it will appear in the job. You

can enter up to six lines. Enter a blank card to end input.

If you do not enter a card, then the Attunity Server default

card is used.

Table 2–10 (Cont.) CICS Adapter Installation Prompts and Responses

Screen Response

Post-Installation Instructions 3-1

3

Post-Installation Instructions

This section describes procedures that are performed after the installation was

successfully performed.

It includes the following topics:

n Overview

n General Post Installation Procedures

n Setting Up Security

n Setting Up Attunity Server to Work with CICS

n Setting Up Attunity Server to Work with IMS/TM

n Setting Up Attunity Server for Reentrancy

n Setting Up Attunity Server to Access DB2 CLI

n Setting Up Attunity Server to Update VSAM Data

n Setting Up Attunity Server to Access IMS/DB

n Installing Attunity Server Natural/CICS Agent

n Setting the Language

Overview

This section describes post instllation tasks that must be performed to work with

Attunity Server.

In addition, if you are upgrading Attunity Server, see Updating an Existing Attunity

Server Installation with CICS.

Attunity Server version for mainframe includes a PS, NAVROOT.DEF.GBLPARMS,

which contains global environment information. This PS is read at startup and the

correct version of Attunity Server is used, based on the details provided in the

Attunity Server startup task.

The information stored in this member includes the dataset qualifier where Attunity

Server is installed, and other information for Attunity Server use.

If you change the location of NAVROOT.DEF.GBLPARMS, you must also change the

relevant cards in the following jobs to the new locations:

n ATTSRVR: Located in an active proclib (such as USER.PROCLIB), as described in

Setting APF-Authorization and Started Tasks.

3-2 Attunity Integration Suite Installation Guide for Mainframe Systems

n ATTDAEMN: Located in an active proclib (such as USER.PROCLIB), as described in

Setting APF-Authorization and Started Tasks.

n NVIMSSRV: Located in an active proclib (such as USER.PROCLIB), as described in

Setting APF-Authorization and Started Tasks.

n NAVSQL: Located in NAVROOT.USERLIB

General Post Installation Procedures

This section includes the following topics:

n Registering Attunity Server

n Setting APF-Authorization and Started Tasks

n Setting 2-Phase Commit

n TCP/IP

n Workspace for z/OS Server Environment File

Registering Attunity Server

Registration is available from within Attunity Server, after adding a machine in the

Design perspective Configuration explorer.

To register Attunity Server

1. In Attunity Studio, right-click the machine and select License Management.

2. Select Register Product.

3. In the Register Product window, browse to the license file supplied by Attunity.

The details of the license are displayed.

4. Click Register to register Attunity Server on this machine.

Setting APF-Authorization and Started Tasks

All JCL jobs and REXX procedures are written to the NAVROOT.USERLIB library. After

the installation procedure completes, do the following:

n Define the LOADAUT library as an APF-authorized library as follows:

1. Enter the following command in the SDSF screen:

"/setprog apf,add,dsn=navroot.loadaut,volume=ac002"

Where ac002 is the volume where you installed Attunity Server and

navroot is the high-level qualifier where Attunity Server is installed.

2. If the Attunity Server installation volume is managed by SMS, then when

defining APF-authorization, enter the following command in the SDSF screen:

"/setprog apf,add,dsn=navroot.loadaut,SMS"

3. Ensure that the library is APF-authorized, even after an IPL of the machine.

Note: The success message that is displayed relates to the license

being loaded to the repository. It does not validate the license itself.

Thus, an invalid license can still generate a success message.

Post-Installation Instructions 3-3

n Move the NAVROOT.USERLIB(ATTDAEMN), NAVROOT.USERLIB(ATTSRVR), and if

you are using IMS/DLI the NAVROOT.USERLIB(NVIMSSRV) members to any

active proclib (such as USER.PROCLIB). ATTDAEMN, ATTSRVR, NVIMSSRV are run

as started tasks.

ATTDAEMN controls the Attunity Server daemon. A daemon runs on every

machine running Attunity Server and manages communication between machines

running Attunity products.

The daemon authenticates clients, authorizes requests for a server process within a

certain server workspace and provides clients with the required servers. When a

client requests a connection, the daemon allocates a server process (or where

applicable, a thread) to handle this connection, and refers the client to the allocated

process.

This may be a new process (dedicated to this client) or an already-started process.

Further communication between the client session and the server process is direct

and does not involve the daemon. The daemon is notified when the connection

ends and the process is either killed or remains available for use by another client.

The server processes are managed by ATTSRVR.

If you decide to rename the ATTSRVR member when you move it to a general

high-level qualifier, then change the name specified in the StartupScript

parameter in the daemon configuration to the new name, as follows:

1. Run NAVROOT.USERLIB(NAVCMD).

2. Enter the following at the prompt:

EDIT DAEMON IRPCDINI

3. Change the startupScript parameter from ATTSRVR to the new name for

the server. For example:

<Workspace name="Navigator"

startupScript="NEW\_NAME"

serverMode="reusable"

... />

4. Exit and save the changes.

5. If you get following error:

ISPS118L SERVICE NOT INVOKED. A VALID ISPF ENVIRONMENT DOES NOT EXIST.

then run the following procedure:

– Run NAVROOT.USERLIB(NAVCMD) and enter ‘export all sys

xml.data.set’ at the prompt.

– Using the z/OS text editor, change the startupScript parameter from

ATTSRVR to the new name for the server. For example:

<Workspace name="Navigator"

startupScript="NEW\_NAME"

serverMode="reusable"

... />

– Rerun NAVROOT.USERLIB(NAVCMD) and enter ‘import sys

xml.data.set’ at the prompt.

3-4 Attunity Integration Suite Installation Guide for Mainframe Systems

n The ATTDAEMN, ATTSRVR, and NVIMSSRV (if you are using IMS/DLI) started

tasks need permission to use an Open Edition TCP/IP stack. The owner must be a

user with OMVS segment defined.

n Change the following line in the ATTDAEMN job to include the IP address of the

z/OS machine.

For example, before:

// PARM=’-B START IRPCDINI’

After:

// PARM='-B -L ip\_address START IRPCDINI'

The following table lists the protected system functions that are used by AIS. AIS

always requires the functions listed for the LOADAUT library. The LOAD library

functions listed require authorization only when you need those functions. See the

Used for: column in the table for an explanation of when and if you need to authorize

the LOAD library.

Setting 2-Phase Commit

To use two-phase commit capability to access data on the z/OS machine, define every

library in the ATTSRVR JCL as an APF-authorized library (see Setting

APF-Authorization and Started Tasks).

TCP/IP

For information about specifying Attunity Server as the service using port 2551 in the

TCP/IP network services file, consult TCP/IP documentation.

Workspace for z/OS Server Environment File

You can configure the daemon server subtask for a workspace through an z/OS

environment file. The file must be named NAVROOT.DEF.workspaceDEF where

NAVROOT is the high level qualifier where Attunity Server is installed. On start up, a

server process for workspace abcd looks for the file NAVROOT.DEF.abcdDEF.

Table 3–1 APF Authorized Functions in AIS

Authorized

Function Library Mandatory Component Used for:

MGCRE LOADAUT Yes Daemon Starting servers by the daemon

RACROUTE LOUDAUT Yes Daemon Authentication of credentials

RACROUTE LOAD No Impersonation Used when a reusable server

needs to impersonate different

users.

MCSOPER, MGCRE LOAD No IMS CDC Used to set up automatic

syncpoints with IMS CDC

IFI functions LOAD No DB2 CDC Using the DB2 instrumentation

facility requires authorization.

RRS LOAD No 2PC Used when setting up two-phase

commit.

Post-Installation Instructions 3-5

The worspaceDEF server environment file has the following format:

<ENVIRONMENT>

SUBSYSTEM=paramvalue1

PLAN=paramvalue2

Setting Up Security

Make the following definitions in the security manager (the following is phrased

sspecifically for RACF, although the same principles also apply to TopSecret and

ACF/II).

Define ATTDAEMN and ATTSRVR with a started task class and a general profile that

enables the following:

n Provide NVIMSSRV access to ATTDAEMN.

n START authority for the ATTSRVR job.

n Access to an Open z/OS segment, which defines access to TCP/IP OE sockets.

n Access for the ATTSRVR.\* profile to the following:

– Adabas: ATTSRVR requires READ authority to the Adabas load library.

– DB2: ATTSRVR requires the following authority:

\* EXECUTE for the used plan.

\* READ, UPDATE, ALTER on the DB2 tables to the level you want to provide

the client application.

You must grant ATTSRVR with READ acess to the sys-tables (SYSTABLES,

SYSCOLUMNS, etc.).

\* TRACE(MON) and MONITOR2 for DB2 CDC.

– IMS/DB and IMS/TM: ATTSRVR requires READ authority for the following

IMS resources:

\* IMSXCF.OTMACI facility.

\* Any facilty defined for the Attunity Server XCF members. For example, on

SY07, if the XCF member is called ATTXCFMB, then set up

IMSXCF.OTMAI07A.ATTXCFMB with READ access in the FACILITY class

and specify the ATTSRVR userid in the access list.

\* IMS.RESLIB

\* IMS.PGMLIB

\* IMS.PROCLIB

n ALTER authority on datasets under NAVROOT (for access to read, write, allocate

and delete under NAVROOT).

Note: If the workspace name is longer than five characters, then the

z/OS environment file name must be truncated to five characters. This

means that the default workspace, Navigator, will look for a file

called NavigDEF.

3-6 Attunity Integration Suite Installation Guide for Mainframe Systems

Attunity Server Stream and DB2 Security

All the libraries in the STEPLIB must be APF-authorized. Grant DB2 DISPLAY

GROUP authorization to the ATTSRVR started task. Issue the following commands to

the owner of the ATTSRVR started task:

GRANT TRACE(STAT)

GRANT TRACE(MON)

GRANT MONITOR2

The owner of the ATTSRVR strarted task must have privileges in DB2 to run offline.

Issue the following command:

-start trace(stat)

Setting Up Attunity Server to Work with CICS

If you did not set up CICS during the installation, do the following to work with CICS:

1. Edit the ATTSRVR member to include the CICS EXCI load library name. ATTSRVR

is located in both NAVROOT.USERLIB and an active proclib (such as

USER.PROCLIB).

For example, edit ATTSRVR to add the following lines:

// DD DSN=&cicspfx.SDFHEXCI,

// DISP=SHR

Where &cicspfx is the CICS system prefix (CICSTS13.CICS for example) and

NAVROOT is the high-level qualifier where Attunity Server is installed.

2. Edit the NAVROOT.USERLIB(NAVCMD) and NAVROOT.USERLIB(NAVSQL) to

include the CICS EXCI load library name to the TASKLIB. For example, add the

following lines:

ALLOCATE DDNAME(TASKLIB) DA('NAVROOT.LOAD'

'&cicspfx.SDFHEXCI' 'ADA622.LOAD'

'ISP.SISPLOAD') SHR

Where &cicspfx is the CICS system prefix (CICSTS13.CICS for example)

NAVROOT is the high-level qualifier where Attunity Server is installed.

3. IRCSTRT=YES must be specified in the CICS initialization parameters, so that the

IRC (Inter Region Communication) starts, as specified in Software Requirements.

4. AIS provides a VTAM netname, ATYCLIEN, for the specific connection used by

EXCI (and MRO) to relay program calls to the CICS target system.

Set up ATYCLIEN as follows:

n Use the JCL in the NAVROOT.USERLIB(CICSCONF) member to submit the

DFHCSDUP batch utility program to add the resource definitions to the

DFHCSD dataset (see the IBM CICS Resource Definition Guide for further

details).

Or,

n Use the instream SYSIN control statements in the

NAVROOT.USERLIB(CICSCONF) member as a guide to defining the resources

online using the CEDA facility.

Post-Installation Instructions 3-7

Setting Up Attunity Server to Work with IMS/TM

In order to execute an IMS transaction with Attunity Server, you need to set OTMA as

described below.

To set OTMA to work with Attunity Server

1. Install OTMA with OTMA C/I where IMS resides, since OTMA is not

automatically installed using the IMS INSTALL/IVP Dialog.

2. In the IMS system definition, set the startup parameter in the IMS procedure to

OTMA=Yes.

In addition, set additional OTMA-related parameters such as GRNAME= for the

XCF group name, and OTMANM= for the IMS member name in that XCF group, as

in the following example:

EDIT IMS.PROCLIB(DFSPBIV1) - 01.03

command ===>

000082 AOIS =,

000083 GRNAME=IMSATT01,

000084 OTMA=YES,

000085 MAXPST=

000086 OTMANM=

3. Start the OTMA Callable Interface (C/I).

4. Add an entry in the program properties table (PPT) for the OTMA C/I

initialization program, by editing the SCHEDxx member of the SYS1.PARMLIB

dataset, and adding the following entry:

PPT PGMNAME(DFSYSVI0)/\*PROGRAM NAME =DFSYSVI0 \*/

CANCEL /\*PROGRAM CAN BE CANCELED \*/

KEY(7) /\*PROTECT KEY ASSIGNED IS 7 \*/

SWAP /\*PROGRAM IS SWAPPABLE \*/

NOPRIV /\*PROGRAM IS NOT PRIVILEGED \*/

DSI /\*REQUIRES DATA SET INTEGRITY \*/

PASS /\*CANNOT BYPASS PASSWORD PROTECTION \*/

SYST /\*PROGRAM IS A SYSTEM TASK \*/

AFF(NONE) /\*NO CPU AFFINITY \*/

NOPREF /\*NO PREFERRED STORAGE FRAMES \*/

5. Do one of the following to make the SCHEDxx changes take effect:

n Re-IPL the system.

n Issue the MVS SET SCH= command.

6. Edit and submit the following JCL procedure to run DFSYSVI0:

//OTMAINIT PROC RGN=3000K,SOUT=A,

/PARM1=

//\*

//IEFPROC EXEC PGM=DFSYSVI0,

//REGION=&RGN

//\*

//STEPLIB DD DISP=SHR,UNIT=SYSDA,

//DSN=IMSVS.RESLIB

//\*

//SYSPRINT DD SYSOUT=&SOUT

//SYSUDUMP DD SYSOUT=&SOUT

//\*

3-8 Attunity Integration Suite Installation Guide for Mainframe Systems

7. Run DFSYSVI0 after the IPL, to initialize OTMA C/I.

Setting up Attunity Server to work with IMS/DB CDC

To ensure that events are written to the log, in the NAVROOT.USERLIB(NVIMSCMD)

the following remove the comment marks (/\*) from the following:

/\* "ALLOCATE DDNAME(IEFRDER) DA('JOHNW.AS5120R."USERID()".TMP.IMSLOG') NEW \*/

/\* DELETE SPACE(1,1) CYL \*/

/\* BLKSIZE(1920) LRECL(1916) RECFM(U) REUSE" \*/

The lines should look like the following:

"ALLOCATE DDNAME(IEFRDER) DA('JOHNW.AS5120R."USERID()".TMP.IMSLOG') NEW

DELETE SPACE(1,1) CYL \*/

BLKSIZE(1920) LRECL(1916) RECFM(U) REUSE"

Setting Up Attunity Server for Reentrancy

All AIS load modules are reentrant to enable subtasking. Therefore, move

INSTROOT.LOAD to the Link Pack Area (LPA).

Where INSTROOT is the high-level qualifier where AIS is installed.

Using the LPA reduces real storage usage (because everyone shares the LPA copy) and

fetch time.

If you intend using impersonation, so that you can run in a security context that is

different than the context of the process that owns the server, then do the following:

1. Place the INSTROOT.LOAD(ATYSVCW) member in an APF-authorized library

outside the LPA.

2. Change the ATTSRVR member (located in the active proclib), by adding the

following to the STEPLIB list:

// DD DSN=apf\_library,DISP=SHR

Where apf\_library is the APF-authorized library outside the LPA where the

ATYSCVW member was moved.

Setting Up Attunity Server to Access DB2 CLI

In order to access DB2 CLI, you must have DB2 CLI installed on the machine. For

details of DB2 CLI, refer to the IBM Call Level Interface Guide and Reference.

The AIS DB2 CLI driver uses an ODBCINI file. During installation of Attunity Server,

an ODBCINI file is defined as a member in NAVROOT.USERLIB.

The ODBCINI file is similar to the following:

; This is a comment line...

; Example COMMON odbcini

[COMMON]

MVSDEFAULTSSID=DSN1

; Example SUBSYSTEM odbcini for DSN1 subsystem

[DSN1]

MVSATTACHTYPE=CAF

PLANNAME=DSNACLI

The PLANNAME value is the default DB2 Calling Level Interface (CLI) plan name. If a

different plan is used, change the name to the correct plan.

Post-Installation Instructions 3-9

You can specify other parameters in the ODBCINI file, as described in the IBM ODBC

Guide and Reference.

You must bind to the plan specified in the PLANNAME parameter. The bind to the plan,

check that the job DSNxxx.SDSNSAMP(DSNTIJCL) includes the following line:

BIND PLAN(DSNACLI)

Where DSNxxx is the DB2 high-level qualifier (the default is DSN610) and DSNACLI is

the plan name specified for the PLANNAME parameter.

For details about setting DB2 security with AIS Stream, see Attunity Server Stream and

DB2 Security.

Setting Up Attunity Server to Update VSAM Data

In order to set up Attunity Server to be able to update VSAM data from a CICS

transaction, copy the UPDTRNS load module from NAVROOT.LOAD to a CICS DFHRPL

library (such as 'CICS.USER.LOAD') and then define the UPDTRNS program under

CICS using any available group such as ATY group:

CEDA DEF PROG(UPDTRNS) G(ATY) LANG(C) DA(ANY) DE(ATTUNIT VSAM UPDATE PROG)

After defining the UPDTRNS program to a group, install it as follows:

CEDA IN G(ATY)

Setting Up Attunity Server to Access IMS/DB

In the NVIMSSRV, NVIMSSQL, NVIMSCMD jobs that call IMS, add DD cards for every

dataset referenced by one of the DBDs for the PSB.

Example 3–1 DD Card

The following DD card can be specified when one of the DBD cards uses the DD card

NAVDD. Note the other cards, which are built based on the entries specified for IMS

during installation.

"ALLOCATE DDNAME(IMS) DA('ATTUNITY.CONNECT.PSBLIB'

'ATTUNITY.CONNECT.DBDLIB') SHR" – location of IMS libraries"ALLOCATE

DDNAME(DFSVSAMP) DA('IMS.PROCLIB(DFSVSMDB)') SHR" – VSAM index file"ALLOCATE

DDNAME(PROCLIB) DA('IMS.PROCLIB') SHR"

Note: In the example, CAF is used, so only one-phase commit

transactions are supported. Attunity Server also supports two-phase

commit transactions, by setting the MVSATTACHTYPE parameter to

RRSAF.

Note: The AUTOCOMMIT initialization parameter is set automatically

by Attunity Server at runtime, and thus should not be set in the

ODBCINI file.

Note: You cannot run multiple versions of NVIMSCMD in the same

session using split screen.

3-10 Attunity Integration Suite Installation Guide for Mainframe Systems

"ALLOCATE DDNAME(NAVDD) DA('ATTUNITY.IMS.DATA.MYDS') SHR" – DD card for data of

the DBD"ALLOCATE DDNAME(IEFRDER) DA('ATTUNITY.CONNECT.TMP.IMSLOG') NEW

DELETE SPACE(1,1) CYL

BLKSIZE(1920) LRECL(1916) RECFM(U) REUSE" – IMS log"CALL

'IMS.RESLIB(DFSRRC00)' 'DLI,NAVUTIL,NAVPSB'" – PSB name for this call

For details about setting up the daemon to work with IMS/DB, see the AIS User Guide

and Reference.

In the security manager, define NVIMSSRV with a started task class and a general

profile that enables the following:

n Access to an Open z/OS segment, that defines access to TCP/IP OE sockets.

n Access to read, write, allocate and delete for datasets under NAVROOT.

Setting Up IMS/DB Under IMS/TM

Perform the following to access IMS/DB data under IMS/TM:

1. Copy the ATYDBDC program from NAVROOT.LOAD to an IMS/TM program library

(such as 'IMS.PGMLIB') with the name of the PSB used to access the IMS/DB data.

2. Define the transaction to point to the program, using statements such as in the

following:

APPLCTN PSB=ATYDBDC,SCHDTYP=PARALLEL

TRANSACT CODE=ATYIMSTM,PRTY=(7,10,2),INQUIRY=NO,MODE=SNGL,EDIT=ULC

The default transaction name is ATYIMSTM. If you use a different transaction, the

transaction name must be less than or equal to eight characters and you must

specify this value in the imsTransname driver property in the binding.

3. Set up OTMA, as described in Setting Up Attunity Server to Work with IMS/TM.

Installing Attunity Server Natural/CICS Agent

The in1stallation copies the following libraries (source and load) and the Natural INPL

dataset to disk:

n A source library (NAVROOT.NATAGENT.SRCLIB).

n A load library (NAVROOT.NATAGENT.LODLIB).

n An INPL dataset containing Natural source programs, object programs, and data

areas (NAVROOT.NATAGENT.INPL).

The following summarizes the installation procedure for the Attunity Server agent for

Natural/CICS Remote Procedure Calls:

1. Configuring the Agent.

2. Installing the CICS Resource Definitions.

3. Loading and Cataloging the Natural Programs.

Note: This DD card is appropriate when using HIDAM.

Note: The above is phrased specifically for RACF, although the same

principles also apply to TopSecret and ACF/II.

Post-Installation Instructions 3-11

4. Making the Agent Load Modules Available to the CICS Region.

5. Verifying the Agent Installation is Successful.

6. Verify the installation is successful from a client machine.

Configuring the Agent

To configure the Natural/CICS Agent

1. Specify the parameters of the Agent Control Block and perform an

Assembly/Link.

See System Parameters for the Natural Agent for a description of all the

parameters available for tailoring the Agent to the specific installation

requirements.

2. Edit the JOBCBLK in the NAVROOT.NATAGENT.SRCLIB source library, as follows:

1. Specify the parameter values you have chosen.

2. Edit dataset names in the assemble/link JCL as appropriate.

3. Submit the job.

4. Check the output to verify that a ATYLCBLK load module has been

successfully link-edited into the LOAD library.

Installing the CICS Resource Definitions

If any program names, transids, etc. were modified in the previous step, edit the

CICSDEF member in the NAVROOT.NATAGENT.SRCLIB source library and make the

appropriate changes to the CICS resource definitions. You may also wish to modify the

RECEIVECOUNT parameter in the ATYS sessions definition (for EXCI communication)

in this member, if the default value (20) is too small for your installation requirements.

The default value set for RECEIVECOUNT is 20.

The CICSDEF member can be used as input to the DFHCSDUP batch utility program to

add the resource definitions to the DFHCSD dataset. A source library member named

JOBCICS with sample JCL has been supplied for convenience. See the IBM CICS

Resource Definition Guide for further details.

For example, edit the LOBCICS member as follows:

//CICSDEF PROC CSDDSN='CICS.DFSCSD',

SRCLIB='NAVROOT.NATAGENT.SRCLIB',

CICSPRF='CICS.CICS'

After editing the file, save and submit it.

Alternatively, the CICSDEF memeber can be used as a guide to defining the resources

online, using the CEDA facility.

After the definitions have been successfully added (either via DFHCSDUP or by manual

online definition), logon to CICS and issue the following commands to install the

resource definitions under CICS:

Note: Specifically, determine which security strategy is best for the

site and how you will implement it. See Parameters for Specific Needs

for information on the SECMODE and AUTO parameters.

3-12 Attunity Integration Suite Installation Guide for Mainframe Systems

CEDA INST GROUP(ATYL)

CEMT SET IRC CLOSE

CEDA INST GROUP(ATYI)

CEMT SET IRC OPEN

Loading and Cataloging the Natural Programs

Either use the JCL contained in JOBNLOAD member in the

NAVROOT.NATAGENT.SRCLIB library, or refer to the in-house Natural administrator,

who should have standard JCL available to load Natural programs from an INPL file

to the Natural user system file using the NATLOAD utility.

Specify the supplied INPL dataset in the JCL (ddname: CMWKF01) and submit the job.

The Natural programs and data areas are loaded to the NATAGENT library on the user

system file. If Natural Security is installed, then the NATAGENT library should be

defined to Natural Security.

Start a Natural online session and perform the following to catalog all of the Attunity

Server programs and data areas:

1. Logon to the NATAGENT library.

2. Issue the CATALL command and enter \* for the program name.

3. Mark the Catalog all Source programs option and press Enter.

4. Add the NATAGENT library to the STEPLIB of all libraries containing subprograms

executed by the Natural agent. Alternatively, move the following four catalogued

modules to SYSTEM library:

n ATYETA

n ATYNDISP

n ATYNDIS2

n ATYPARMS

Making the Agent Load Modules Available to the CICS Region

Make the Natural agent load modules available to the CICS region in one of following

ways:

n Concatenate the agent load library to the DFHRPL ddname in the CICS region JCL.

n Copy the required load modules to a user load library already defined in DFHRPL.

If the CICS region is currently active, the NEWCOPY function of CEMT must be

executed to make the load modules accessible for this session of CICS.

Note: For Natural version 2.3 and higher, use the NATLOAD utility

instead of the INPL utility.

Note: The TESTAG01 source subprogram is used to verify a

successful installation. This subprogram should have been cataloged

after performing the previous steps.

Post-Installation Instructions 3-13

As a rule, peruse the list of resources being defined to CICS in the CICSDEF member

in the Natural agent source library (programs, transactions, connections, etc.) and

decide what to authorize in order for the Natural agent to work.

In particular note that the ATYN, ATYP, and ATYM transactions are all being started as

asynchronous non-terminal tasks and should be defined to the security tool (such as

RACF) accordingly. Also the ATYCLIEN special connection for EXCI should be defined

to the security tool.

Verifying the Agent Installation is Successful

Test remote procedure calls are included in the kit to verify a successful installation.

The two remote procedure calls perform simple arithmetic manipulations on the input

parameters and return the results as output parameters.

The first test verifies that the ATY transaction and the Natural agent function correctly.

The second verifies that the Attunity Server can be used with Natural.

To verify the installation on the Mainframe is successful

1. Edit the TESTINST member in the provided source library and make any

necessary changes. In particular, change the &APPLID variable to the value of

APPLID in the CICS region.

2. Save the member.

3. Edit the JOBAGENT member in the provided source libraries and make any

necessary changes for the site. In particular, set the TESTNUM variable to 01.

4. Submit the job.

The JOBLOG of the batch job should show the following results:

+RESP = 00000000

+RESP2 = 00000000

+ABCODE =

+OPERAND1 = 0128

+OPERAND2 = 0016

+SUM = 00144

+DIFFERENCE = 0112

+PRODUCT = 00002048

+QUOTIENT = 0008

+ERRCODE = 00000000

+MESSAGE = TESTAG01 EXECUTED SUCCESSFULLY

Note: Be cautioned that the ATYN transaction is not intended to be

issued directly from a terminal, and will usually terminate abnormally

when issued from a terminal (It is designed to be attached and

executed asynchronously as a non-terminal background task by the

Natural agent).

Note: Other variables enable you to modify the arithmetic operands

and find-criteria of the subprograms being called. Do not change these

variables when initially verifying the installation.

3-14 Attunity Integration Suite Installation Guide for Mainframe Systems

Verifying the Installation is Successful from a Client

Test remote procedure calls are included in the kit to verify a successful installation.

These remote procedure calls perform simple arithmetic manipulations on the input

parameters and return the results as output parameters.

To verify the installation is successful from a client machine

1. Specify an entry in the binding configuration similar to the following:

<datasources>

<datasource name=’NATPROC’ type=’NATURAL’

connect=’CICS,ATYCLIEN’ />

</datasources>

2. Set up the metadata for the TESTAG01 procedure. The XML definition for the

metadata is as follows:

<?xml version='1.0'?>

<navobj>

<procedure name="testag01">

<dbCommand>

PROGRAM=ATYLSTN;TRANSID=ATYI;LIBRARY=NATAGENT

SUBPROGRAM=TESTAG01

</dbCommand>

<fields>

<field name="SUM" datatype="ada\_numstr\_s" size="5" scale="0"/>

<field name="DIFFERENCE" datatype="ada\_numstr\_s" size="4"

scale="0"/>

<field name="PRODUCT" datatype="ada\_numstr\_s" size="8" scale="0"/>

<field name="QUOTIENT" datatype="ada\_numstr\_s" size="4"

scale="0"/>

</fields>

<parameters>

<field name="OPERAND1" datatype="ada\_numstr\_s" size="4" scale="0"/>

<field name="OPERAND2" datatype="ada\_numstr\_s" size="4" scale="0"/>

</parameters>

</procedure>

</navobj>

3. Import the ADD metadata XML file to Attunity Server by running the NAVCMD

IMPORT utility. For example:

Run NAVROOT.USERLIB (NAVCMD) and enter ’IMPORT NATPROC

NATAGENT.SAMPLE.ADD.TSTAG01X’ at the prompt, where

NATAGENT.SAMPLE.ADD.TSTAG01X is the dataset which contains the XML

Note: The following error is commonly received (on the JOBLOG)

when the APPLID in the TESTINST member has not been set

properly:

RESP = 00000008

RESP2 = 00000203

If you receive this error, return to step 1 above and set the name of the

CICS APPLID correctly, then re-submit. If you still receive the error,

make sure that the specified CICS region is in fact active.

Post-Installation Instructions 3-15

4. Execute calls from a client to confirm that the software is functioning as specified.

For example, on a non-z/OS machine, running Attunity Server, use NAV\_UTIL

EXECUTE NATPROC.

n TESTAG01: Receives two arithmetic operands and returns their sum,

difference, product and quotient.

n Input parameters: OPERAND1 (numeric, 4 bytes,0 precision), OPERAND2

(numeric, 4 bytes, 0 precision).

n Output parameters: SUM (numeric, 5 bytes, 0 precision), DIFFERENCE

(numeric, 4 bytes, 0 precision), PRODUCT (numeric, 8 bytes, 0 precision),

QUOTIENT (numeric, 4 bytes, 0 precision).

Example 3–2

Set the input parameters as follows:

OPERAND1=128

OPERAND2=16

The following output parameters should be returned:

SUM=144

DIFFERENCE=112

PRODUCT=2048

QUOTIENT=8

Setting the Language

National Language Support (NLS) is provided by Attunity Server for the following

languages:

n English (the default)

n Hebrew

n Japanese

n Korean

n Simple Chinese

n Traditional Chinese

The language is specified in the following Attunity Server environment settings:

n language

n codepage

For more information on NLS, see "National Language Support (NLS)" in the AIS User

Guide and Reference.

3-16 Attunity Integration Suite Installation Guide for Mainframe Systems

Index-1

Index

Numerics

2PC, 3-4

2-Phase Commit, 3-4

A

AIS Server registration, 3-2

APF-Authorization

setting, 3-2

C

Cataloging

Natural programs, 3-12

Codepage

setting, 3-15

D

disk space requirements

IBM S/390, 2-1

H

hardware requirements

IBM S/390 disk space, 2-1

UNIX, 2-1

I

IBM S/390

postinstallation, 2-9

preinstallation, 2-3

IBM z/OS

installation, 2-4

importing installation kit, 2-3

installation

IBM z/OS, 2-4

importing kit, 2-3

kit, 2-3

Installing

CICS resource definitions, 3-11

K

kit installation, 2-3

L

License, 3-2

Loading

Natural programs, 3-12

N

Natural programs

cataloging, 3-12

installing, 3-12

O

operating system requirements

UNIX, 2-1

P

postinstallation

IBM S/390, 2-9

preinstallation

IBM S/390, 2-3

processor requirements

UNIX, 2-1

R

Reentrancy, 3-8

Registering, 3-2

requirements

UNIX hardware requirements, 2-1

UNIX software requirements, 2-1

S

Security

setting up, 3-5

Server Environment File, 3-4

Setting

apf-authorization, 3-2

language, 3-15

security, 3-5

Setting Up

CICS, 3-6

DB2 CLI, 3-8

IMS/DB, 3-9

Index-2

IMS/TM, 3-7

updating VSAM data, 3-9

software requirements

UNIX operating system, 2-1

Started Tasks, 3-2

T

TCP/IP, 3-4

V

Verifying

from a client machine, 3-14

successful installation, 3-13

VSAM Data, 3-9